

2. Manually configure static routes on a router to direct packets to different subnets. Use the ip


route command and verify connectivity using ping and traceroute.


Topology :




IP Configuration :













Static Route with IP route:









Ping and traceroute Test ::

